Connecting Multiple VTI LED Posters

# Connecting Hardware

Below familiarize yourself with your LED Poster’s basic input and output ports.

A diagram of a computer

Description automatically generated­­­

A green arrow pointing to a white box

Description automatically generated

## Multi-Screen Display

To connect two or more LED Posters, you simply need to connect the “HDMI OUT” of Poster1 to the “HDMI IN” of Poster2. (see right)

|  |  |
| --- | --- |
| **Poster1: HDMI OUT** | **Poster2: HDMI IN** |
| **A close-up of a cable plugged into a black device  Description automatically generated** | **A close up of a device  Description automatically generated** |
| Seamless Video Wall To fit LED Posters together for **a seamless Video Wall** you only need to:   1. Remove the magnetic sidebars (see right) between two posters. 2. Station LED Posters next to each other (see below). | A white rectangular object with red arrows  Description automatically generated |

1. A close-up of a green circuit board

   Description automatically generatedRemove the modules between two posters, which cover the \*sidelock of the Poster cabinet

|  |  |
| --- | --- |
| A black rectangular object with green and white squares  Description automatically generated | 5***Use magnet included in LED Poster kit.*** |

\*Side locks (pictured below)

1. Wrench the side lock and screws as shown in the attached video.

Close-up of a machine with a red arrow

Description automatically generated

1. A green arrow pointing to a white box


   Description automatically generatedConnect the Poster1 HDMI OUT to the Poster2 HDMI IN.

## Display Content - Viplex Handy


1. Connect to Screen
   1. Click Set Network to access the WLAN connection page of the mobile phone.
   2. Connect the WiFi AP of Taurus series products. (The default SSID is the last 8 digits of AP+SN, and the password is 12345678.)

A screenshot of a phone

Description automatically generated

1. Run ViPlex Handy Mobile App

|  |  |
| --- | --- |
| **Android** | **iOS** |
| [Download Link](https://play.google.com/store/apps/details?id=%20nova.priv.hand.easypluto.google) | [Download Link](https://apps.apple.com/us/app/viplexhandy/id%201241302188) |
|  | |

1. xs
2. Enter Device Management

A screenshot of a phone

Description automatically generated

1. A screenshot of a phone

   Description automatically generatedSelect the Multi-Screen Mosaic
   1. Steps (shown in Red Numbering above):
      1. 1) Setting of splicing direction; (If the software is connected to the leftmost poster, choose the direction from left to right (facing the screen))
      2. 2) Splicing method: according to the width or according to the number, we choose "quantity"
      3. 3) The number of splicing should be consistent with the number of screens.
      4. 4) Press “Done”.